## Designer Liners, LLC 610-321-0260

**D/b/a Designer Tub & Tile (888) 639-9988**

 As seen on HGTV’s Real Estate Intervention **101 Fellowship Rd. #195**

 **Uwchland, PA 19480**

**Job** **Proposal/Invoice** Fully Insured

Date of Estimate/Job \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Client Source\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Name \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Address \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ City\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Zip\_\_\_\_\_\_

Phone (H) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ (W) \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**We will thoroughly clean, prep, sand, chemical bond and resurface areas listed below:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| AREA | NUMBER OF COATS | GLOSS LEVEL | COLOR | COMMENTS | PRICE |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |

 **TOTAL** \_\_\_\_\_\_\_\_\_\_\_

Payment is due in full upon job completion.

Special Instructions/Other Comments:

All work is to be completed in a professional manner according to standard practices. Any alteration or deviation from above specifications may result in a charge over and above the estimate. Warranties are as stated on reverse side.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

SIGNATURE OF AGENT SIGNATURE OF HOMEOWNER

 \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 JOB COMPLETED

**IMPORTANT: PLEASE READ AND FOLLOW CARE**

**INSTRUCTIONS AND WARRANTY INFORMATION ON BACK PAGE.**

HIC#PA040968

This Is The Best Reglazing System...Period!

**Care and Maintenance Instructions**

**First 24 hours** - Do not use the reglazed surface for 24 hours. Ensure that dirt and debris do not fall on the wet and tacky surface by staying away from the sprayed areas. After the 24 hour dry time remove any masking tape the tech has left, by scoring with a razor blade first, than removing. Recaulk if applicable.

**Cure time** - In the first 2 to 3 weeks the sprayed areas are still adhering and hardening, so extra care should be taken.

**Cleaners** - Do not use abrasive cleaners or bleaches. We recommend any foam, such as Scrubbing Bubbles, sprays such as Formula 409, or gels. "Gelgloss" brand is recommended for any hard water or calcium stain areas. Clean as needed or staining may damage sprayed areas.

**Bathmats** - Do not use bathmats or stick-on appliqués. The only slip resistant surface we recommend is our spray on slip resistant finish, for which there is a nominal fee. Ask the tech for details.

**Leaks** - Fix all dripping faucets ASAP.

**Shampoo** - Do not leave soap or bottles on the surface where water will collect, for long periods of time. This is especially important during the cure time. Shake shower curtains to remove excess moisture.

**Chemicals** - Never let chemicals such as dyes, drain openers or bleach stand on the surface.

**Caulk** - Always keep the sprayed surface grouted and caulked as needed.

**If the surface is damaged, call this office immediately.** We may repair the area involved or resurface the entire unit (at our discretion).

**Warranty**

Designer Tub & Tile warranties, for chipping and peeling only, the surfaces of bathtubs and wall tile reglazed by us in owner occupied housing for a period of 5 years providing the customer has maintained the surface as recommended. During the first 2 years, repairs due to defects in material or workmanship will be made free of charge. During the balance of the warranty period there will be a charge of 50% of the cost for the required service. Rust, corrosion, spot repairs, and all other surfaces are not warranted. Bathtubs and tile for commercial, rental, or contractor accounts are warranted for one year. A travel charge may be applied.

**Designer Tub & Tile ... 610-321-0260**